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声光电视讯系统产品                                                               高新技术企业
Receiver T-591U(s)
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Description 
[bookmark: _GoBack]It is a digital wireless microphone system with a new solution architecture. The system adopts digital U-band transmission technology, pi/4-DQPSK modulation mode, and uses ID code pilot technology to prevent cross-frequency interference, and frequency sweep to avoid interference, characterized by low bit error rate, stable transmission, and strong anti-interference ability. It can be widely used in conferences, training, public broadcasting, large-scale parties and other places.

Feature 
*  Adopt unique digital U-band transmission technology, pi/4-DQPSK modulation mode, strong anti-interference ability, low bit error rate and stable transmission.
*  Adopting a unique encryption method for audio transmission to protect the content of the meeting.
*  Adopting unique ID code foreign frequency technology can prevent frequency interference.
*  Support one-click frequency scanning to avoid interference; one-click infrared frequency matching, easy to operate.
*  Support reverb, high, middle and bass adjustments.
*  Support one channel of balanced output and one channel of unbalanced output.
*  The receiver uses a 2.2-inch TFT-LCD screen to display information more delicately.
*  The receiver panel is made with exquisite craftsmanship and is elegant and beautiful.
*  The transmitting power is adjustable, adjust the transmitting power as needed.

Specification
	Frequency range
	540MHz-590MHz、640MHz-690MHz

	Receive sensitivity
	＜-95dBm

	THD+N
	＜0.1%

	Maximum output
	Balanced output 500mV, unbalanced output 1000mV，unbalanced MIC output 50mV

	SNR
	≥105dB（XLR）

	Channels
	≥16

	Frequency response
	20Hz~20KHz ±3dB

	Dynamic range
	≥115dB

	Antenna interface
	BNC/impedance 50 ohms

	Power supply
	DC 12V/1A

	Working current
	≤300mA

	Dimensions (D×W×H)
	214×223.5×52mm

	Weight
	1.32kg



Model Configuration Explanation

* T-591U – Standard Configuration
This is the standard version normally shown in the general product datasheet.
* T-591U(s) – Special Factory Configuration
* This is the same T-591U product family and the same basic equipment platform, but supplied from the factory with additional or enhanced technical characteristics available according to the customer's project requirements.
* The important point is that T-591U remains the main model family. The letters (s) only identify the specific factory configuration supplied under that model.
因产品不断升级改进，本图册所提供的产品图片及技术参数等仅供参考，请以产品实物为准
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