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High-tech enterprise of audio-visual television communication system products
Touchscreen  TS-9110 A(s)
New Central Control Editing Software V1.0
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Product Introduction
This is a 10.1-inch capacitive touch all-in-one machine developed based on the Android system. The display screen is a 10.1-inch high-definition display with a resolution of 1280*800, providing delicate picture quality. It has a built-in 200W camera and speaker, supports PoE power supply, and can communicate and control with the central control system. It also has indicator lights to provide feedback on different scenarios. It is suitable for various mid-to-high-end conference rooms, control centers, and other occasions, making it a high-end human-machine interface device.

Features
1. Thin body, overall thickness 27mm, one-piece high-precision molded middle frame.
2. It has a built-in 200W camera and 2*1W speakers .
3. Two RJ45 network interfaces, supporting gigabit network transmission.
4. Supports multi-touch on capacitive screens.
5. Full-view HD screen with a resolution of 1280*800 .
6. It supports PoE power supply, simplifying wiring.
7. Supports DC12V/2.6A power supply.

Technical parameters
	CPU
	RK3568, quad-core 64-bit, Cortex-A55, 2.0GHz

	RAM
	LPDDR-2G

	Memory
	EMMC-16G has a built-in (expandable TF card) slot.

	operating system
	Android 11.0

	Display screen
	LED backlit LCD screen (Grade A)

	resolution
	1280*800

	Visible area
	216.5*135 mm

	Contrast
	2000:1

	brightness
	300cd/m2

	screen ratio
	16:10

	touchscreen
	10.1-inch capacitive touchscree, supports 10-point touch mode, response speed ≤3ms

	LED strip
	I/O port protocol, built-in seven-color LED light strip

	Media Playback
	Video formats: MPEG-1, MPEG-2, MPEG-4, H.263, H.264, VC1, RV
Audio formats: MP3/WMA/AAC
Image format: jpeg

	trumpet
	8Ω 1W×2

	Camera
	200W front camera

	Communication interface
	One 10M/100M/1000M adaptive Ethernet

	Back-out interface
	Supports both Ethernet and RS-485 serial ports on the back, suitable for embedded installation.

	Side control interface
	Dry contact NO/NC/COM interface

	Other interfaces
	Two external USB 3.0 ports (one of which is USB_OTG).

	WiFi/3G/4G/Bluetooth
	Supports WIFI-2.4G and BT-4.1.

	POE
	Supported by IEEE 802.3at/af

	powered by
	Supports PoE/DC12V power supply

	Overall power consumption
	≤12W

	standby power consumption
	≤1W

	Operating temperature
	-5℃～45℃ (Screen operating temperature is 0℃-40℃)

	Operating temperature
	0℃-40℃

	Operating humidity
	30%～85%

	Storage temperature
	-10℃～50℃

	Storage humidity
	10%～90%

	[bookmark: _GoBack]Altitude
	Below 2000 meters

	color
	silver

	Gross weight (packaging)
	2kg

	[bookmark: OLE_LINK1]Packaging size (width × height × thickness)
	309*270*55mm

	Weight
	1.3kg

	Dimensions (L×W×D) mm
	253.5*163.5*30mm



Model Configuration Clarification 
- The ITC TS-9110A product family is available in different factory configurations according to the technical specifications required for each order. The model TS-9110A identifies the standard configuration, while the model TS-9110A(s) identifies the factory-enhanced configuration that incorporates additional technical features installed by the manufacturer. Both configurations belong to the same TS-9110A product family and use the same base product platform.
- The letters (s) are factory configuration identifiers within the TS-9110A product family and are used for ordering, production, and product traceability purposes. The configuration letter does not represent a different product family.
- For this project, the TS-9110A system will be supplied in the TS-9110A(s) factory configuration, incorporating the following additional required technical features.
Due to continuous product upgrades and improvements, the product images and technical specifications provided in this catalog are for reference only. Please refer to the actual product for the most accurate representation.
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